Hide navigation sidebar
Hide table of contents sidebar
Back to top
Toggle table of contents sidebar

# frame_transfer.h

void ma_frame_tx(const chanend_t c_frame_out, const int32_t frame[], const unsigned channel_count, const unsigned sample_count)

  Transmit 32-bit PCM frame over a channel.

  This function transmits the 32-bit PCM frame `frame[]` over the channel `c_frame_out`.

  This is a blocking call which will wait for a receiver to accept the data from the channel. Typically this will be accomplished with a call to `ma_frame_rx()` or `ma_frame_rx_transpose()`.

  The receiver is not required to be on the same tile as the sender.

  Note

  Internally, a channel transaction is established to reduce the overhead of channel communication. Any custom functions are used to receive this frame in an application, they must wrap the channel reads in a (slave) channel transaction. See `xcore/channel_transaction.h`.

  Warning

  No protocol is used to ensure consistency between the frame layout of the transmitter and receiver. Disagreement about frame size will likely cause one side to block indefinitely. It is the responsibility of the application author to ensure consistency between transmitter and receiver.

  Parameters:

    - c_frame_out – Channel over which to send frame.

    - frame – Frame to be transmitted.

    - channel_count – Number of channels represented in the frame.

    - sample_count – Number of samples represented in the frame.

void ma_frame_rx(int32_t frame[], const chanend_t c_frame_in, const unsigned channel_count, const unsigned sample_count)

  Receive 32-bit PCM frame over a channel.

  This function receives a PCM frame over `c_frame_in`. Normally, the frame will have been transmitted using `ma_frame_tx()`. The received frame is stored in `frame[]`.

  This is a blocking call which does not return until the frame has been fully received.

  The sender is not required to be on the same tile as the receiver.

  Note

  Internally, a channel transaction is established to reduce the overhead of channel communication. This function may only be used to receive the frame if the transmitter has wrapped the channel writes in a (master) channel transaction. See `xcore/channel_transaction.h`.

  Warning

  No protocol is used to ensure consistency between the frame layout of the transmitter and receiver. Disagreement about frame size will likely cause one side to block indefinitely. It is the responsibility of the application author to ensure consistency between transmitter and receiver.

  Parameters:

    - frame – Buffer to store received frame.

    - c_frame_in – Channel from which to receive frame.

    - channel_count – Number of channels represented in the frame.

    - sample_count – Number of samples represented in the frame.

void ma_frame_rx_transpose(int32_t frame[], const chanend_t c_frame_in, const unsigned channel_count, const unsigned sample_count)

  Receive 32-bit PCM frame over a channel with transposed dimensions.

  This function receives a PCM frame over `c_frame_in`. Normally, the frame will have been transmitted using `ma_frame_tx()`. The received frame is stored in `frame[]`.

  Unlike `ma_frame_rx()`, this function reorders the frame elements as they are received. `ma_frame_tx()` always transmits the frame elements in memory order. This function swaps the channel and sample axes so that if the transmitter frame has shape `(CHANNEL, SAMPLE)`, the caller’s frame array will have shape `(SAMPLE, CHANNEL)`.

  This is a blocking call which does not return until the frame has been fully received.

  The sender is not required to be on the same tile as the receiver.

  Note

  Internally, a channel transaction is established to reduce the overhead of channel communication. This function may only be used to receive the frame if the transmitter has wrapped the channel writes in a (master) channel transaction. See `xcore/channel_transaction.h`.

  Warning

  No protocol is used to ensure consistency between the frame layout of the transmitter and receiver. Disagreement about frame size will likely cause one side to block indefinitely. It is the responsibility of the application author to ensure consistency between transmitter and receiver.

  Parameters:

    - frame – Buffer to store received frame.

    - c_frame_in – Channel from which to receive frame.

    - channel_count – Number of channels represented in the frame.

    - sample_count – Number of samples represented in the frame.