Hide navigation sidebar
Hide table of contents sidebar
Back to top
Toggle table of contents sidebar

# SPI RTOS Driver

This driver can be used to instantiate and control a SPI master or slave mode I/O interface on xcore in an RTOS application.

- SPI Master RTOS Driver
  - SPI Master Initialization API
  - SPI Master Core API
  - SPI Master RPC Initialization API
- SPI Slave RTOS Driver
  - SPI Slave API