Hide navigation sidebar
Hide table of contents sidebar
Back to top
Toggle table of contents sidebar

# Supported Hardware

This example application is supported on the XK-VOICE-L71 board.

## Setting up the Hardware

This example design requires an XTAG4 and XK-VOICE-L71 board.

### xTAG

The xTAG is used to program and debug the device

Connect the xTAG to the debug header, as shown below.

Connect the micro USB XTAG4 and micro USB XK-VOICE-L71 to the programming host.