Hide navigation sidebar
Hide table of contents sidebar
Skip to content
Back to top
Toggle table of contents sidebar

# Custom decimation filters

In the `TwoStageDecimator`, the tap count and decimation factor for the first stage decimator are fixed to `256` and `32` respectively, as described in Decimator stage 1.

These parameters cannot be changed without implementing a custom decimator, which is outside the scope of this document.

However, both the first-stage and second-stage filter coefficients may be replaced, and the second-stage decimation factor and tap count may be freely modified by running the mic array component with custom filters. This is described in the following sections.

## Designing a custom filter

A filter design script is provided in `python/filter_design/design_filter.py`. The script contains functions to generate the filters currently provided as part of `lib_mic_array` and save them as `.pkl` files. Using these functions as a guide, the script can be extended to generate custom filters tailored to the application’s needs.

Note that in `TwoStageDecimator`, both the first and second stage filters are implemented using fixed-point arithmetic, which requires the coefficients to be presented in a specific format. The helper scripts `python/stage1.py` and `python/stage2.py` generate the correctly quantized and interleaved coefficient arrays required by the library.

After generating a `.pkl` file, the helper scripts `stage1.py` and `stage2.py` can be used to format the first and second stage filters, respectively, into the fixed-point C arrays required by the library.

Alternatively, the `combined.py` script can process both the first and second stage filters in one step. When executed, `stage1.py`, `stage2.py`, and `combined.py` print the filter coefficients as C-style arrays, along with filter-related defines such as tap count, decimation factor, etc., as `#define` macros on stdout.

The scripts can also be run with the `--file-prefix <prefix>` (or `-fp <prefix>`) option. In this mode, all arrays and defines are written into a header file (`<prefix>.h`), which can be included in the application.

Running `python combined.py --help` from the `python` directory shows full usage instructions.

From the `python` directory, the workflow is typically:

    python filter_design/design_filter.py                     # generates the
                                                              # .pkl files
    python combined.py <custom_filter.pkl> -fp <prefix>      # converts the
                                                              # .pkl file to C
                                                              # arrays for stage
                                                              # 1 and 2, and
                                                              # writes to
                                                              # <prefix>.h

## Using custom filters

When using the `TwoStageDecimator` provided by the library, the `mic_array_init_custom_filter()` function is used to initialize a mic array instance with a custom 2-stage decimation filter.

Note

The custom filter provided to `mic_array_init_custom_filter()` must be compatible with the `TwoStageDecimator` requirements. Specifically, it must be a 2-stage filter. The tap count and decimation factor for the first-stage decimator are fixed at `256` and `32`, respectively, and the filter must be compatible with the Filter implementation (Stage 1).

The second-stage decimation filter tap count and decimation ratio are flexible, provided it is a standard FIR filter compatible with Filter implementation (Stage 2). Using custom filters that are incompatible with the implementation in `TwoStageDecimator` is outside the scope of this documentation.

The `mic_array_conf_t` structure is populated with the decimator and PDM RX configurations before calling `mic_array_init_custom_filter()`. In particular, the application must:

- Allocate all filter coefficient buffers, filter state buffers, and PDM RX buffers referenced by the decimator and PDM RX configurations, and ensure they persist for the lifetime of the mic array instance (until `mic_array_start()` returns).

- Populate the decimator pipeline configuration (`mic_array_decimator_conf_t`) and the PDM RX configuration (`pdm_rx_conf_t`) structures.

Note

When designing custom filters as described in Designing a custom filter, the filter coefficient arrays and associated configuration parameters can be written to a header file by running `combined.py`. This file is included in the application, and the decimation filter coefficients and other parameters in `mic_array_filter_conf_t` are populated from it.

The application must still allocate persistent runtime buffers for the filter delay line (`mic_array_filter_conf_t`) and for the PDM RX input and output buffers (`pdm_rx_conf_t`).

Below is a snippet from the app_custom_filter source code showing how the `mic_array_conf_t` structure is populated:

    #include "good_2_stage_filter.h" // Autogenerated by running 'python combined.py filter_design/good_2_stage_filter_int.pkl -fp good_2_stage_filter'

    void init_mic_conf(mic_array_conf_t &mic_array_conf, mic_array_filter_conf_t (&filter_conf)[2], unsigned *channel_map)
    {
      static int32_t stg1_filter_state[APP_MIC_COUNT][8];
      static int32_t stg2_filter_state[APP_MIC_COUNT][GOOD_2_STAGE_FILTER_STG2_TAP_COUNT];
      memset(&mic_array_conf, 0, sizeof(mic_array_conf_t));

      //decimator
      mic_array_conf.decimator_conf.filter_conf = &filter_conf[0];
      mic_array_conf.decimator_conf.num_filter_stages = 2;
      // filter stage 1
      filter_conf[0].coef = (int32_t*)good_2_stage_filter_stg1_coef;
      filter_conf[0].num_taps = GOOD_2_STAGE_FILTER_STG1_TAP_COUNT;
      filter_conf[0].decimation_factor = GOOD_2_STAGE_FILTER_STG1_DECIMATION_FACTOR;
      filter_conf[0].state = (int32_t*)stg1_filter_state;
      filter_conf[0].shr = GOOD_2_STAGE_FILTER_STG1_SHR;
      filter_conf[0].state_words_per_channel = filter_conf[0].num_taps/32; // works on 1-bit samples
      // filter stage 2
      filter_conf[1].coef = (int32_t*)good_2_stage_filter_stg2_coef;
      filter_conf[1].num_taps = GOOD_2_STAGE_FILTER_STG2_TAP_COUNT;
      filter_conf[1].decimation_factor = GOOD_2_STAGE_FILTER_STG2_DECIMATION_FACTOR;
      filter_conf[1].state = (int32_t*)stg2_filter_state;
      filter_conf[1].shr = GOOD_2_STAGE_FILTER_STG2_SHR;
      filter_conf[1].state_words_per_channel = GOOD_2_STAGE_FILTER_STG2_TAP_COUNT;

      // pdm rx
      static uint32_t pdmrx_out_block[APP_MIC_COUNT][GOOD_2_STAGE_FILTER_STG2_DECIMATION_FACTOR];
      static uint32_t __attribute__((aligned(8))) pdmrx_out_block_double_buf[2][APP_MIC_COUNT * GOOD_2_STAGE_FILTER_STG2_DECIMATION_FACTOR];
      mic_array_conf.pdmrx_conf.pdm_out_words_per_channel = GOOD_2_STAGE_FILTER_STG2_DECIMATION_FACTOR;
      mic_array_conf.pdmrx_conf.pdm_out_block = (uint32_t*)pdmrx_out_block;
      mic_array_conf.pdmrx_conf.pdm_in_double_buf = (uint32_t*)pdmrx_out_block_double_buf;
      mic_array_conf.pdmrx_conf.channel_map = channel_map;
    }

Once `mic_array_conf_t` is populated, mic array can be initialised by calling `mic_array_init_custom_filter()` and started by calling `mic_array_start()`:

    unsigned channel_map[2] = {0,1};
    mic_array_conf_t mic_array_conf;
    mic_array_filter_conf_t filter_conf[2];
    init_mic_conf(mic_array_conf, filter_conf, channel_map);
    mic_array_init_custom_filter(&pdm_res, &mic_array_conf);

    par {
      mic_array_start((chanend_t) c_audio_frames);

      <... other tasks ...>
    }

Note

Apart from calling `mic_array_init_custom_filter()` instead of `mic_array_init()`, all other aspects of using the custom filter API, such as including the mic array in an application, declaring resources, and overriding build-time default configuration, are exactly the same as in the default usage model described in Using lib_mic_array.