Hide navigation sidebar
Hide table of contents sidebar
Skip to content
Back to top
Toggle table of contents sidebar

# S/PDIF receive

The codebase supports a single, stereo, S/PDIF receiver. This can be input via 75 Ω coaxial or optical fibre. In order to provide S/PDIF functionality `lib_xua` uses lib_spdif.

Basic configuration of S/PDIF receive functionality is achieved with the defines in Table 17

Table 17 S/PDIF rx defines
Define | Description | Default
--- | --- | ---
`XUA_SPDIF_RX_EN` | Enable S/PDIF receive | `0` (Disabled)
`SPDIF_RX_INDEX` | Defines which channels S/PDIF will be input on | N/A (must be defined)

Note

S/PDIF receive always runs on the tile defined by `AUDIO_IO_TILE`

The codebase expects the S/PDIF receive port to be defined in the application XN file as `PORT_SPDIF_IN`. This must be a 1-bit port, for example:

    <Port Location="XS1_PORT_1A"  Name="PORT_SPDIF_IN"/>

When S/PDIF receive is enabled the codebase expects to either drive a synchronisation signal to an external Cirrus Logic CS2100 device or use lib_sw_pll (xcore.ai only) for master-clock generation.

The programmer should ensure the defines in Table 18 are set appropriately

Table 18 Reference clock location
Define | Description | Default
--- | --- | ---
`PLL_REF_TILE` | Tile location of reference to CS2100 device | `AUDIO_IO_TILE`

The codebase expects this reference signal port to be defined in the application XN file as `PORT_PLL_REF`. This may be a port of any bit-width, however, connection to bit[0] is assumed:

    <Port Location="XS1_PORT_1A"  Name="PORT_PLL_REF"/>

Configuration of the external CS2100 device (typically via I2C) is beyond the scope of this document.