Hide navigation sidebar
Hide table of contents sidebar
Skip to content
lib_xua: USB Audio components library v5.3.0
view PDF:

- Overview
- Software architecture
- Basic usage
- Options
  Toggle navigation of Options
  - Strings
  - Code Location
  - Channel Counts and Sample Rates
  - USB Audio Class Support
  - Synchronisation
  - I2S/TDM
  - S/PDIF Transmit
  - S/PDIF Receive
  - ADAT Transmit
  - ADAT Receive
  - MIDI
  - PDM Microphones
  - Mixer
  - Direct Stream Digital (DSD)
  - DFU
  - USB Audio Formats
  - Other Options
- Advanced usage
  Toggle navigation of Advanced usage
  - Core hardware resources
  - Running the core components
  - I2S/TDM
  - Mixer
- Additional features
  Toggle navigation of Additional features
  - S/PDIF transmit
  - S/PDIF receive
  - ADAT transmit
  - ADAT receive
- Implementation detail
  Toggle navigation of Implementation detail
  - Audio Hub and I²S
  - Endpoint 0: Management and control
  - Audio endpoints (Endpoint Buffer and Decoupler)
  - XMOS USB Device (XUD) library
  - External clock recovery (Clock Gen)
  - Digital mixer
  - S/PDIF transmit
  - S/PDIF receive
  - MIDI
  - PDM microphones
  - Audio controls via Human Interface Device (HID)
  - Device Firmware Upgrade (DFU) over USB
  - Resource usage
- API
  Toggle navigation of API
  - Configuration defines
  - User function definitions
  - Component API

Back to top
Toggle table of contents sidebar